(kicad_symbol_lib
  (version 20211014)
  (generator https://github.com/uPesy/easyeda2kicad.py)
  (symbol "FT232RL-REEL"
    (in_bom yes)
    (on_board yes)
    (property
      "Reference"
      "U"
      (id 0)
      (at 0 33.02 0)
      (effects (font (size 1.27 1.27) ) )
    )
    (property
      "Value"
      "FT232RL-REEL"
      (id 1)
      (at 0 -33.02 0)
      (effects (font (size 1.27 1.27) ) )
    )
    (property
      "Footprint"
      "lcsc_lib:SSOP-28_L10.2-W5.3-P0.65-LS7.8-BL"
      (id 2)
      (at 0 -35.56 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (property
      "Datasheet"
      "https://lcsc.com/product-detail/USB_FTDI_FT232RL-REEL_FT232RL-REEL_C8690.html"
      (id 3)
      (at 0 -38.10 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (property
      "LCSC Part"
      "C8690"
      (id 5)
      (at 0 -40.64 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (symbol "FT232RL-REEL_0_1"
      (rectangle
        (start -17.78 22.86)
        (end 17.78 -22.86)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin unspecified line
        (at 22.86 -20.32 180)
        (length 5.08)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 22.86 -17.78 180)
        (length 5.08)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line
        (at 2.54 27.94 270)
        (length 5.08)
        (name "VCCIO" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 22.86 17.78 180)
        (length 5.08)
        (name "RXD" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 22.86 2.54 180)
        (length 5.08)
        (name "RI" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line
        (at 0.00 -27.94 90)
        (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 22.86 12.70 180)
        (length 5.08)
        (name "DSR" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 22.86 5.08 180)
        (length 5.08)
        (name "DCD" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 22.86 7.62 180)
        (length 5.08)
        (name "CTS" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line
        (at 22.86 -12.70 180)
        (length 5.08)
        (name "CBUS4" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line
        (at 22.86 -7.62 180)
        (length 5.08)
        (name "CBUS2" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line
        (at 22.86 -10.16 180)
        (length 5.08)
        (name "CBUS3" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line
        (at -22.86 7.62 0)
        (length 5.08)
        (name "USBDP" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line
        (at -22.86 12.70 0)
        (length 5.08)
        (name "USBDM" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin output line
        (at -22.86 20.32 0)
        (length 5.08)
        (name "3V3OUT" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line
        (at 2.54 -27.94 90)
        (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -22.86 -2.54 0)
        (length 5.08)
        (name "RESET" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line
        (at -2.54 27.94 270)
        (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line
        (at 5.08 -27.94 90)
        (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line
        (at 22.86 -5.08 180)
        (length 5.08)
        (name "CBUS1" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line
        (at 22.86 -2.54 180)
        (length 5.08)
        (name "CBUS0" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line
        (at -5.08 -27.94 90)
        (length 5.08)
        (name "AGND" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -22.86 -20.32 0)
        (length 5.08)
        (name "TEST" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -22.86 -7.62 0)
        (length 5.08)
        (name "OSCI" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin output line
        (at -22.86 -15.24 0)
        (length 5.08)
        (name "OSCO" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin output line
        (at 22.86 20.32 180)
        (length 5.08)
        (name "TXD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line
        (at 22.86 15.24 180)
        (length 5.08)
        (name "DTR" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line
        (at 22.86 10.16 180)
        (length 5.08)
        (name "RTS" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SP485EEN-L_TR"
    (in_bom yes)
    (on_board yes)
    (property
      "Reference"
      "U"
      (id 0)
      (at 0 8.89 0)
      (effects (font (size 1.27 1.27) ) )
    )
    (property
      "Value"
      "SP485EEN-L/TR"
      (id 1)
      (at 0 -8.89 0)
      (effects (font (size 1.27 1.27) ) )
    )
    (property
      "Footprint"
      "lcsc_lib:SOIC-8_L5.0-W4.0-P1.27-LS6.0-BL"
      (id 2)
      (at 0 -11.43 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (property
      "Datasheet"
      "https://lcsc.com/product-detail/RS-485-RS-422_SIPEX_SP485EEN-L-TR_SP485EEN-L-TR_C6855.html"
      (id 3)
      (at 0 -13.97 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (property
      "LCSC Part"
      "C6855"
      (id 5)
      (at 0 -16.51 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (symbol "SP485EEN-L_TR_0_1"
      (rectangle
        (start -5.08 6.35)
        (end 5.08 -6.35)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin unspecified line
        (at -10.16 3.81 0)
        (length 5.08)
        (name "RO" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -10.16 1.27 0)
        (length 5.08)
        (name "~{RE}" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -10.16 -1.27 0)
        (length 5.08)
        (name "DE" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -10.16 -3.81 0)
        (length 5.08)
        (name "DI" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 10.16 -3.81 180)
        (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 10.16 -1.27 180)
        (length 5.08)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 10.16 1.27 180)
        (length 5.08)
        (name "B" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 10.16 3.81 180)
        (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "DC-005-5A-2.0"
    (in_bom yes)
    (on_board yes)
    (property
      "Reference"
      "DC"
      (id 0)
      (at 0 7.62 0)
      (effects (font (size 1.27 1.27) ) )
    )
    (property
      "Value"
      "DC-005-5A-2.0"
      (id 1)
      (at 0 -7.62 0)
      (effects (font (size 1.27 1.27) ) )
    )
    (property
      "Footprint"
      "lcsc_lib:DC-IN-TH_DC-005-5A-2.0"
      (id 2)
      (at 0 -10.16 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (property
      "Datasheet"
      "https://lcsc.com/product-detail/New-Arrivals_XKB-Enterprise-DC-005-5A-2-0_C381116.html"
      (id 3)
      (at 0 -12.70 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (property
      "LCSC Part"
      "C381116"
      (id 5)
      (at 0 -15.24 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (symbol "DC-005-5A-2.0_0_1"
      (rectangle
        (start -2.54 4.06)
        (end -1.52 1.02)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (arc
        (start -7.62 -1.52)
        (mid -7.41 -1.55)
        (end -7.62 -3.56)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.00 2.54) (xy -1.52 2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 3.56) (xy -7.62 3.56)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 1.52) (xy -7.62 1.52)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.00 -2.54) (xy -7.37 -2.54) (xy -7.87 -1.52) (xy -8.38 -2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.00 -0.00) (xy -4.32 -0.00) (xy -4.32 -2.54) (xy -4.57 -1.27)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -4.32 -2.54) (xy -4.06 -1.27)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (pin unspecified line
        (at 5.08 2.54 180)
        (length 5.08)
        (name "1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 5.08 -2.54 180)
        (length 5.08)
        (name "2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 5.08 -0.00 180)
        (length 5.08)
        (name "3" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "HYCW445-USBC16-730B"
    (in_bom yes)
    (on_board yes)
    (property
      "Reference"
      "USB"
      (id 0)
      (at 0 17.78 0)
      (effects (font (size 1.27 1.27) ) )
    )
    (property
      "Value"
      "HYCW445-USBC16-730B"
      (id 1)
      (at 0 -20.32 0)
      (effects (font (size 1.27 1.27) ) )
    )
    (property
      "Footprint"
      "lcsc_lib:USB-TYPE-C-SMD_TYPE-C-16P-USB616FC"
      (id 2)
      (at 0 -22.86 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (property
      "LCSC Part"
      "C42400246"
      (id 5)
      (at 0 -25.40 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (symbol "HYCW445-USBC16-730B_0_1"
      (rectangle
        (start -10.16 16.51)
        (end 7.62 -17.78)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (circle
        (center -8.89 13.97)
        (radius 0.38)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (pin unspecified line
        (at -12.70 12.70 0)
        (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "A1B12" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -12.70 10.16 0)
        (length 2.54)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "A4B9" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -12.70 7.62 0)
        (length 2.54)
        (name "CC1" (effects (font (size 1.27 1.27))))
        (number "A5" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -12.70 5.08 0)
        (length 2.54)
        (name "DP1" (effects (font (size 1.27 1.27))))
        (number "A6" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -12.70 2.54 0)
        (length 2.54)
        (name "DN1" (effects (font (size 1.27 1.27))))
        (number "A7" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -12.70 -0.00 0)
        (length 2.54)
        (name "SBU1" (effects (font (size 1.27 1.27))))
        (number "A8" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -12.70 -2.54 0)
        (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "B1A12" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -12.70 -5.08 0)
        (length 2.54)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "B4A9" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -12.70 -7.62 0)
        (length 2.54)
        (name "CC2" (effects (font (size 1.27 1.27))))
        (number "B5" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -12.70 -10.16 0)
        (length 2.54)
        (name "DP2" (effects (font (size 1.27 1.27))))
        (number "B6" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -12.70 -12.70 0)
        (length 2.54)
        (name "DN2" (effects (font (size 1.27 1.27))))
        (number "B7" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -12.70 -15.24 0)
        (length 2.54)
        (name "SBU2" (effects (font (size 1.27 1.27))))
        (number "B8" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 12.70 2.54 180)
        (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 12.70 -0.00 180)
        (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 12.70 -2.54 180)
        (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 12.70 -5.08 180)
        (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "USBLC6-2P6"
    (in_bom yes)
    (on_board yes)
    (property
      "Reference"
      "D"
      (id 0)
      (at 0 12.70 0)
      (effects (font (size 1.27 1.27) ) )
    )
    (property
      "Value"
      "USBLC6-2P6"
      (id 1)
      (at 0 -12.70 0)
      (effects (font (size 1.27 1.27) ) )
    )
    (property
      "Footprint"
      "lcsc_lib:SOT-666-6_L1.6-W1.2-P0.50-LS1.6-BR"
      (id 2)
      (at 0 -15.24 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (property
      "Datasheet"
      "https://lcsc.com/product-detail/Diodes-ESD_STMicroelectronics_USBLC6-2P6_USBLC6-2P6_C15999.html"
      (id 3)
      (at 0 -17.78 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (property
      "LCSC Part"
      "C15999"
      (id 5)
      (at 0 -20.32 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (symbol "USBLC6-2P6_0_1"
      (rectangle
        (start -10.16 12.70)
        (end 10.16 -12.70)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (circle
        (center 0.00 3.81)
        (radius 0.25)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle
        (center 0.00 -3.81)
        (radius 0.25)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle
        (center 7.87 -0.00)
        (radius 0.25)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle
        (center -7.62 -0.00)
        (radius 0.25)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc
        (start 0.25 -7.62)
        (mid 0.25 -7.61)
        (end 0.25 -7.62)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc
        (start 0.25 7.62)
        (mid 0.25 7.63)
        (end 0.25 7.62)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc
        (start 0.00 -3.81)
        (mid 0.05 -3.56)
        (end 0.00 -3.81)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.16 7.62) (xy 10.16 7.62)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.16 -7.62) (xy 10.16 -7.62)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 5.08) (xy -2.54 3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 3.81) (xy -2.54 2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 5.08) (xy 5.08 3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 3.81) (xy 5.08 2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 -2.54) (xy -2.54 -3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 -3.81) (xy -2.54 -5.08)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 -2.54) (xy 5.08 -3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 -3.81) (xy 5.08 -5.08)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 1.27) (xy 1.27 -0.00)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 -0.00) (xy 1.27 -1.27)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.78 1.27) (xy 1.27 1.27)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 1.27) (xy 1.27 -0.00)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 -0.00) (xy 1.27 -1.27)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 -1.27) (xy 0.51 -1.27)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.00 7.62) (xy 0.00 3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 3.81) (xy 2.54 3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 3.81) (xy -7.62 3.81) (xy -7.62 -3.81) (xy -5.08 -3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.16 -0.00) (xy -7.62 -0.00)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 -3.81) (xy 2.54 -3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 4.83 -3.81) (xy 7.87 -3.81) (xy 7.87 3.81) (xy 5.08 3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 7.87 -0.00) (xy 10.16 -0.00)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.00 -7.62) (xy 0.00 -3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -7.62 -0.00) (xy 7.87 -0.00)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 2.54) (xy -2.54 3.81) (xy -5.08 5.08) (xy -5.08 2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 2.54 2.54) (xy 5.08 3.81) (xy 2.54 5.08) (xy 2.54 2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -5.08 -5.08) (xy -2.54 -3.81) (xy -5.08 -2.54) (xy -5.08 -5.08)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 2.54 -5.08) (xy 5.08 -3.81) (xy 2.54 -2.54) (xy 2.54 -5.08)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -1.27 -1.27) (xy 1.27 -0.00) (xy -1.27 1.27) (xy -1.27 -1.27)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin input line
        (at -15.24 7.62 0)
        (length 5.08)
        (name "I/O1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line
        (at -15.24 -0.00 0)
        (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line
        (at -15.24 -7.62 0)
        (length 5.08)
        (name "I/O2" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line
        (at 15.24 -7.62 180)
        (length 5.08)
        (name "I/O2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line
        (at 15.24 -0.00 180)
        (length 5.08)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line
        (at 15.24 7.62 180)
        (length 5.08)
        (name "I/O1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
)