(kicad_symbol_lib
  (version 20211014)
  (generator https://github.com/uPesy/easyeda2kicad.py)
  (symbol "USBLC6-2P6"
    (in_bom yes)
    (on_board yes)
    (property
      "Reference"
      "D"
      (id 0)
      (at 0 12.70 0)
      (effects (font (size 1.27 1.27) ) )
    )
    (property
      "Value"
      "USBLC6-2P6"
      (id 1)
      (at 0 -12.70 0)
      (effects (font (size 1.27 1.27) ) )
    )
    (property
      "Footprint"
      "lcsc_lib:SOT-666-6_L1.6-W1.2-P0.50-LS1.6-BR"
      (id 2)
      (at 0 -15.24 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (property
      "Datasheet"
      "https://lcsc.com/product-detail/Diodes-ESD_STMicroelectronics_USBLC6-2P6_USBLC6-2P6_C15999.html"
      (id 3)
      (at 0 -17.78 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (property
      "LCSC Part"
      "C15999"
      (id 5)
      (at 0 -20.32 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (symbol "USBLC6-2P6_0_1"
      (rectangle
        (start -10.16 12.70)
        (end 10.16 -12.70)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (circle
        (center 0.00 3.81)
        (radius 0.25)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle
        (center 0.00 -3.81)
        (radius 0.25)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle
        (center 7.87 -0.00)
        (radius 0.25)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (circle
        (center -7.62 -0.00)
        (radius 0.25)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc
        (start 0.25 -7.62)
        (mid 0.25 -7.61)
        (end 0.25 -7.62)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc
        (start 0.25 7.62)
        (mid 0.25 7.63)
        (end 0.25 7.62)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc
        (start 0.00 -3.81)
        (mid 0.05 -3.56)
        (end 0.00 -3.81)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.16 7.62) (xy 10.16 7.62)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.16 -7.62) (xy 10.16 -7.62)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 5.08) (xy -2.54 3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 3.81) (xy -2.54 2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 5.08) (xy 5.08 3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 3.81) (xy 5.08 2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 -2.54) (xy -2.54 -3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 -3.81) (xy -2.54 -5.08)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 -2.54) (xy 5.08 -3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 -3.81) (xy 5.08 -5.08)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 1.27) (xy 1.27 -0.00)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 -0.00) (xy 1.27 -1.27)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.78 1.27) (xy 1.27 1.27)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 1.27) (xy 1.27 -0.00)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 -0.00) (xy 1.27 -1.27)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 -1.27) (xy 0.51 -1.27)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.00 7.62) (xy 0.00 3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 3.81) (xy 2.54 3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 3.81) (xy -7.62 3.81) (xy -7.62 -3.81) (xy -5.08 -3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.16 -0.00) (xy -7.62 -0.00)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 -3.81) (xy 2.54 -3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 4.83 -3.81) (xy 7.87 -3.81) (xy 7.87 3.81) (xy 5.08 3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 7.87 -0.00) (xy 10.16 -0.00)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.00 -7.62) (xy 0.00 -3.81)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -7.62 -0.00) (xy 7.87 -0.00)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 2.54) (xy -2.54 3.81) (xy -5.08 5.08) (xy -5.08 2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 2.54 2.54) (xy 5.08 3.81) (xy 2.54 5.08) (xy 2.54 2.54)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -5.08 -5.08) (xy -2.54 -3.81) (xy -5.08 -2.54) (xy -5.08 -5.08)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 2.54 -5.08) (xy 5.08 -3.81) (xy 2.54 -2.54) (xy 2.54 -5.08)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -1.27 -1.27) (xy 1.27 -0.00) (xy -1.27 1.27) (xy -1.27 -1.27)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin input line
        (at -15.24 7.62 0)
        (length 5.08)
        (name "I/O1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line
        (at -15.24 -0.00 0)
        (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line
        (at -15.24 -7.62 0)
        (length 5.08)
        (name "I/O2" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line
        (at 15.24 -7.62 180)
        (length 5.08)
        (name "I/O2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line
        (at 15.24 -0.00 180)
        (length 5.08)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line
        (at 15.24 7.62 180)
        (length 5.08)
        (name "I/O1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
)