(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/A")
	(net 2 "GND")
	(net 3 "/B")
	(net 4 "+5V")
	(net 5 "unconnected-(U1-CBUS4-Pad12)")
	(net 6 "unconnected-(U1-USBDM-Pad16)")
	(net 7 "unconnected-(U1-DTR-Pad2)")
	(net 8 "unconnected-(U1-RESET-Pad19)")
	(net 9 "unconnected-(U1-DSR-Pad9)")
	(net 10 "unconnected-(U1-RTS-Pad3)")
	(net 11 "unconnected-(U1-OSCI-Pad27)")
	(net 12 "unconnected-(U1-CTS-Pad11)")
	(net 13 "unconnected-(U1-CBUS1-Pad22)")
	(net 14 "unconnected-(U1-RI-Pad6)")
	(net 15 "unconnected-(U1-CBUS0-Pad23)")
	(net 16 "unconnected-(U1-NC-Pad8)")
	(net 17 "unconnected-(U1-NC-Pad24)")
	(net 18 "unconnected-(U1-DCD-Pad10)")
	(net 19 "unconnected-(U1-USBDP-Pad15)")
	(net 20 "unconnected-(U1-OSCO-Pad28)")
	(net 21 "unconnected-(U1-3V3OUT-Pad17)")
	(net 22 "Net-(U1-RXD)")
	(net 23 "Net-(U1-CBUS3)")
	(net 24 "Net-(U1-CBUS2)")
	(net 25 "Net-(U1-TXD)")
	(net 26 "unconnected-(FB1-Pad1)")
	(net 27 "unconnected-(FB1-Pad2)")
	(footprint "lcsc_lib:SSOP-28_L10.2-W5.3-P0.65-LS7.8-BL"
		(layer "F.Cu")
		(uuid "2c64b921-6e68-464a-9c73-cc21730d590d")
		(at 26.58 87.54)
		(property "Reference" "U1"
			(at 0 -7.46 0)
			(layer "F.SilkS")
			(uuid "c0d30c6e-9c70-4ee5-b3e6-5d3899c2220b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "FT232RL-REEL"
			(at 0 7.46 0)
			(layer "F.Fab")
			(uuid "6b0eace7-7809-4035-8743-6de603bcc3b0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://lcsc.com/product-detail/USB_FTDI_FT232RL-REEL_FT232RL-REEL_C8690.html"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "947e6b8d-2da9-45b1-af6f-932e81f90724")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7b672e76-7568-4bff-931a-8aafa8cb22cc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC Part" "C8690"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "475df633-c849-401f-a87a-f97c59a723b3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/174e2ee6-7177-43e5-821a-87ef081c0c70")
		(sheetname "/")
		(sheetfile "pcb_dock.kicad_sch")
		(attr smd)
		(fp_line
			(start -5.08 -2.2)
			(end 5.08 -2.2)
			(stroke
				(width 0.25)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "86466309-e38a-4593-b754-b60050465b82")
		)
		(fp_line
			(start -5.08 -0.63)
			(end -5.08 -2.2)
			(stroke
				(width 0.25)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d06b1d06-f994-47bd-8e50-36893502d436")
		)
		(fp_line
			(start -5.08 0.64)
			(end -5.08 2.2)
			(stroke
				(width 0.25)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e53412ca-af3e-4caa-ab18-9efbbae26fee")
		)
		(fp_line
			(start -5.08 2.2)
			(end 5.08 2.2)
			(stroke
				(width 0.25)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a1bc305b-4977-4064-b297-45e4bb4eb326")
		)
		(fp_line
			(start 5.08 -2.2)
			(end 5.08 2.16)
			(stroke
				(width 0.25)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "077a96c0-f363-4bf9-9bea-4ef9f6ba8156")
		)
		(fp_arc
			(start -5.08 -0.63)
			(mid -4.524941 0.000797)
			(end -5.081582 0.630199)
			(stroke
				(width 0.25)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9d9eea85-6de4-4eb9-a266-6b64bb356970")
		)
		(fp_circle
			(center -4.23 4.28)
			(end -4.08 4.28)
			(stroke
				(width 0.3)
				(type solid)
			)
			(fill no)
			(layer "Cmts.User")
			(uuid "8bb0f7e2-3d1b-4736-9f62-2d51a6db64ff")
		)
		(fp_circle
			(center -4.06 1.4)
			(end -4.03 1.4)
			(stroke
				(width 0.06)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "c806d896-4a1d-42db-a8b8-633f81d20f87")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d0287f5f-4b34-4588-906d-6d1b397fdae1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd oval
			(at -4.23 3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(U1-TXD)")
			(pinfunction "TXD")
			(pintype "output")
			(uuid "53b701ae-7eda-4855-830a-fdbaff27e1e9")
		)
		(pad "2" smd oval
			(at -3.58 3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "unconnected-(U1-DTR-Pad2)")
			(pinfunction "DTR")
			(pintype "output")
			(uuid "2c4cd3b5-8b02-43cf-a790-7975c3673bd2")
		)
		(pad "3" smd oval
			(at -2.93 3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "unconnected-(U1-RTS-Pad3)")
			(pinfunction "RTS")
			(pintype "output")
			(uuid "4fc59e5d-17c5-4bd1-bd33-dc36d1c51038")
		)
		(pad "4" smd oval
			(at -2.28 3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "+5V")
			(pinfunction "VCCIO")
			(pintype "power_in")
			(uuid "f97f01d0-5630-44f2-96df-888b7cbe28e0")
		)
		(pad "5" smd oval
			(at -1.63 3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "Net-(U1-RXD)")
			(pinfunction "RXD")
			(pintype "unspecified")
			(uuid "03e26b9c-d71f-4ea0-84f8-d3e180985b5b")
		)
		(pad "6" smd oval
			(at -0.98 3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "unconnected-(U1-RI-Pad6)")
			(pinfunction "RI")
			(pintype "unspecified")
			(uuid "99ae5af6-50eb-469d-a200-3c135d73f7ef")
		)
		(pad "7" smd oval
			(at -0.32 3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "17664e4d-3068-4cf5-a9ed-bb107b80e849")
		)
		(pad "8" smd oval
			(at 0.33 3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "unconnected-(U1-NC-Pad8)")
			(pinfunction "NC")
			(pintype "unspecified")
			(uuid "b82dc853-ba1c-48fb-8cd3-be85d32ecd8d")
		)
		(pad "9" smd oval
			(at 0.98 3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "unconnected-(U1-DSR-Pad9)")
			(pinfunction "DSR")
			(pintype "unspecified")
			(uuid "49c413f9-c0da-47b9-bb7f-49026fee1e0d")
		)
		(pad "10" smd oval
			(at 1.63 3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "unconnected-(U1-DCD-Pad10)")
			(pinfunction "DCD")
			(pintype "unspecified")
			(uuid "d980ff37-fbfb-4de9-9107-a919c4db5f03")
		)
		(pad "11" smd oval
			(at 2.28 3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "unconnected-(U1-CTS-Pad11)")
			(pinfunction "CTS")
			(pintype "unspecified")
			(uuid "6b86f1c4-ec12-4730-9113-966d45a30e53")
		)
		(pad "12" smd oval
			(at 2.93 3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "unconnected-(U1-CBUS4-Pad12)")
			(pinfunction "CBUS4")
			(pintype "bidirectional")
			(uuid "0f75d0ba-a673-4cca-9261-388f32d090b0")
		)
		(pad "13" smd oval
			(at 3.58 3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U1-CBUS2)")
			(pinfunction "CBUS2")
			(pintype "bidirectional")
			(uuid "46d799de-763f-4e28-aa4c-fb8e021eee7a")
		)
		(pad "14" smd oval
			(at 4.23 3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(U1-CBUS3)")
			(pinfunction "CBUS3")
			(pintype "bidirectional")
			(uuid "40c9fda4-c0c4-466f-9b3b-f3c74550e144")
		)
		(pad "15" smd oval
			(at 4.23 -3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "unconnected-(U1-USBDP-Pad15)")
			(pinfunction "USBDP")
			(pintype "bidirectional")
			(uuid "db577468-65f1-40e3-ba30-b8cc18808a86")
		)
		(pad "16" smd oval
			(at 3.58 -3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "unconnected-(U1-USBDM-Pad16)")
			(pinfunction "USBDM")
			(pintype "bidirectional")
			(uuid "1325ba95-c85d-43fe-8936-93cc0c5de1ea")
		)
		(pad "17" smd oval
			(at 2.93 -3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "unconnected-(U1-3V3OUT-Pad17)")
			(pinfunction "3V3OUT")
			(pintype "output")
			(uuid "fcf43723-fc8c-4c45-9318-77f418a86451")
		)
		(pad "18" smd oval
			(at 2.28 -3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "7de8b431-210e-47ae-83f0-7319867b2b4c")
		)
		(pad "19" smd oval
			(at 1.63 -3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "unconnected-(U1-RESET-Pad19)")
			(pinfunction "RESET")
			(pintype "unspecified")
			(uuid "402fcf16-d7b6-4fca-bf53-663bb21c1f0d")
		)
		(pad "20" smd oval
			(at 0.98 -3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
			(uuid "4c37e618-494c-4371-bdeb-18cc665182dc")
		)
		(pad "21" smd oval
			(at 0.33 -3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "4217ed3b-2d2d-4c4a-b678-158f566d263a")
		)
		(pad "22" smd oval
			(at -0.32 -3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "unconnected-(U1-CBUS1-Pad22)")
			(pinfunction "CBUS1")
			(pintype "bidirectional")
			(uuid "909c02a9-1e4f-43fe-99c9-b33c3a02ad2e")
		)
		(pad "23" smd oval
			(at -0.98 -3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "unconnected-(U1-CBUS0-Pad23)")
			(pinfunction "CBUS0")
			(pintype "bidirectional")
			(uuid "ae9cf324-85b8-4473-9ca9-44d8a50f1e66")
		)
		(pad "24" smd oval
			(at -1.63 -3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "unconnected-(U1-NC-Pad24)")
			(pinfunction "NC")
			(pintype "unspecified")
			(uuid "d704f055-e8cf-4a35-bf4f-81e411b8120d")
		)
		(pad "25" smd oval
			(at -2.28 -3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "AGND")
			(pintype "power_in")
			(uuid "852206d7-453b-4ca5-b05b-90520c2b5af4")
		)
		(pad "26" smd oval
			(at -2.93 -3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "TEST")
			(pintype "unspecified")
			(uuid "4aa79ff3-297c-4b27-875b-33e971456355")
		)
		(pad "27" smd oval
			(at -3.58 -3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "unconnected-(U1-OSCI-Pad27)")
			(pinfunction "OSCI")
			(pintype "unspecified")
			(uuid "53841860-a344-44de-a775-f246be8df336")
		)
		(pad "28" smd oval
			(at -4.23 -3.46)
			(size 0.36 2.02)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "unconnected-(U1-OSCO-Pad28)")
			(pinfunction "OSCO")
			(pintype "output")
			(uuid "e739d42a-c227-422b-9f9e-d3d723529658")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/lib/lcsc_lib.3dshapes/SSOP-28_L10.2-W5.3-H2.0-LS7.8-P0.65.wrl"
			(offset
				(xyz 0 -0 -0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "summitwave_dock_connector:MG0425BME"
		(layer "F.Cu")
		(uuid "59303395-3cb7-4194-8f61-badeb3813716")
		(at 110.23 70.73)
		(property "Reference" "J2"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "057a1f76-ff98-4c71-9298-1453e7d4957a")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "Conn_01x04"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "061b940c-87c7-430c-8c5e-f6c50c4af0f3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9510376c-726a-431f-beb7-c974c1b1b4ad")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d73908d0-d950-4f43-8971-f22b9a172733")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/6234d344-4b55-4a3c-b808-6b7854e5275d")
		(sheetname "/")
		(sheetfile "pcb_dock.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.61 -12.11)
			(end -0.23 -12.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e3c4de2f-5227-4b80-98e0-7074c539c2ca")
		)
		(fp_line
			(start -1.61 -10.73)
			(end -1.61 -12.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eff3648b-e33c-4b46-b21b-377297e20463")
		)
		(fp_line
			(start -1.61 -9.46)
			(end -1.61 -1.73)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ba2cda41-6000-45ad-b76d-032313c6b672")
		)
		(fp_line
			(start -1.61 -9.46)
			(end 1.15 -9.46)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "17143cc2-bd6f-48b1-98be-5f1de0499c95")
		)
		(fp_line
			(start -1.61 -1.73)
			(end 1.15 -1.73)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2a5b0564-5a4d-4be6-a877-e0b646160c43")
		)
		(fp_line
			(start 1.15 -9.46)
			(end 1.15 -1.73)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4746dbdf-dd84-4a9e-b34a-8ffe29567f14")
		)
		(fp_line
			(start -2 -12.5)
			(end -2 -1.34)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b4d23e47-0bff-4caa-8e76-42ae89df0efe")
		)
		(fp_line
			(start -2 -1.34)
			(end 1.54 -1.34)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6a4c98a7-5ae4-4887-abd2-14886913380d")
		)
		(fp_line
			(start 1.54 -12.5)
			(end -2 -12.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8e0c50b5-64e6-466a-924f-9ed3bd2121de")
		)
		(fp_line
			(start 1.54 -1.34)
			(end 1.54 -12.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4f00b8c0-8a68-411a-93c2-0c9a903941c0")
		)
		(fp_line
			(start -1.5 -11.365)
			(end -0.865 -12)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b764b00c-4c1e-4b9b-9e75-ba126eb665c6")
		)
		(fp_line
			(start -1.5 -1.84)
			(end -1.5 -11.365)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e7f9d326-fc07-42be-9a79-a822856dabeb")
		)
		(fp_line
			(start -0.865 -12)
			(end 1.04 -12)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "56d9153a-b5b8-49e4-ac25-dad24841fd0e")
		)
		(fp_line
			(start 1.04 -12)
			(end 1.04 -1.84)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d9e22b6e-8771-4db7-9964-16b0a2d6fcd9")
		)
		(fp_line
			(start 1.04 -1.84)
			(end -1.5 -1.84)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "348caa17-22da-48a9-97bd-aa43f921cb76")
		)
		(fp_text user "${REFERENCE}"
			(at -0.23 -6.92 90)
			(layer "F.Fab")
			(uuid "dc128777-7ed5-4b77-8333-e8643a69d8b5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "f47d7d25-c098-4a49-979a-579435033361")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at -0.23 -10.73)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "51db4b20-0a1f-4bb0-aad9-6cb3f67986dc")
		)
		(pad "2" thru_hole circle
			(at -0.23 -8.19)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/A")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "bb1011e9-d315-4384-999c-6e4ad8083498")
		)
		(pad "3" thru_hole circle
			(at -0.23 -5.65)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/B")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "23611361-d3fd-4993-b2ef-7b9079e08075")
		)
		(pad "4" thru_hole circle
			(at -0.23 -3.11)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "c972e4e9-bbe8-4d5e-919a-c7ef30654b07")
		)
		(embedded_fonts no)
		(embedded_files
			(file
				(name "MG0425BME.pdf")
				(type datasheet)
				(checksum "DDC9158D3DB55A592FB92759BC04B6F0")
			)
		)
		(model "${KIPRJMOD}/lib/MG0425BME.STEP"
			(offset
				(xyz -2.23 6.915 1.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "summitwave_dock_connector:MG0425BME"
		(layer "F.Cu")
		(uuid "792d86ee-e000-4177-97e4-703fa4c7e545")
		(at 50.23 70.73)
		(property "Reference" "J1"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "c20264d1-be6e-42e7-b456-5c25cc5d9998")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "Conn_01x04"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "736d87cc-fd4d-48d4-bb73-0f80d21f4faa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9374f74d-4842-40d7-ad60-99b2d52c53df")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dcc354fe-fd6b-4114-9178-a74b51f81579")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/85327688-ffb5-4b50-9b7e-86337e4925fc")
		(sheetname "/")
		(sheetfile "pcb_dock.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.61 -12.11)
			(end -0.23 -12.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4596f449-9054-415f-91ef-e88971d63452")
		)
		(fp_line
			(start -1.61 -10.73)
			(end -1.61 -12.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e6280170-afa6-41fa-a383-45a5bb5fd3b4")
		)
		(fp_line
			(start -1.61 -9.46)
			(end -1.61 -1.73)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4b74c384-abaa-4260-a06c-1c53bb56ee64")
		)
		(fp_line
			(start -1.61 -9.46)
			(end 1.15 -9.46)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b793e204-d854-4cff-bc28-03e0cc1ff4a5")
		)
		(fp_line
			(start -1.61 -1.73)
			(end 1.15 -1.73)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "78d284c8-97ea-457c-8e87-ae2dbab32352")
		)
		(fp_line
			(start 1.15 -9.46)
			(end 1.15 -1.73)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "516a4006-0f97-45aa-9d6d-88a5ed1575fb")
		)
		(fp_line
			(start -2 -12.5)
			(end -2 -1.34)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4fc4445d-9c1a-4acf-8a2e-8d0d61bc0689")
		)
		(fp_line
			(start -2 -1.34)
			(end 1.54 -1.34)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dfce2b2f-423a-4f8f-899b-88eb2230227e")
		)
		(fp_line
			(start 1.54 -12.5)
			(end -2 -12.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "54173d9c-7f3a-4927-b2f3-64ea9f5f8514")
		)
		(fp_line
			(start 1.54 -1.34)
			(end 1.54 -12.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1f8b426e-8435-4fff-b282-d5e7c3c648a2")
		)
		(fp_line
			(start -1.5 -11.365)
			(end -0.865 -12)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aaca01a0-5ac7-4a0c-8176-36cfbdf0e214")
		)
		(fp_line
			(start -1.5 -1.84)
			(end -1.5 -11.365)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1e53ec86-447e-41f6-887f-53d9c6aa2e7b")
		)
		(fp_line
			(start -0.865 -12)
			(end 1.04 -12)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1f729bad-b9e2-434b-9f1b-dc3458ca7c02")
		)
		(fp_line
			(start 1.04 -12)
			(end 1.04 -1.84)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1b31f863-d36e-4047-a6d4-cb3597da7c9a")
		)
		(fp_line
			(start 1.04 -1.84)
			(end -1.5 -1.84)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "52b3f27f-860f-4684-af54-20980b3cf2d1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "90fb0980-ba4b-435c-8bc6-de79c054fd95")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "${REFERENCE}"
			(at -0.23 -6.92 90)
			(layer "F.Fab")
			(uuid "e0c92eb7-c754-4aec-9ab6-3063b2a5b328")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at -0.23 -10.73)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "bbb78f8e-7f3d-43a5-81aa-6ef98eef84a2")
		)
		(pad "2" thru_hole circle
			(at -0.23 -8.19)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/A")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "2359b5d1-e3bc-47be-b494-c180e60a04cd")
		)
		(pad "3" thru_hole circle
			(at -0.23 -5.65)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/B")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "62f88f8f-5e3f-4dbe-8062-cf1271b3b072")
		)
		(pad "4" thru_hole circle
			(at -0.23 -3.11)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "455d0b5c-8794-49bf-a995-1bddef2f00fe")
		)
		(embedded_fonts no)
		(embedded_files
			(file
				(name "MG0425BME.pdf")
				(type datasheet)
				(checksum "DDC9158D3DB55A592FB92759BC04B6F0")
			)
		)
		(model "${KIPRJMOD}/lib/MG0425BME.STEP"
			(offset
				(xyz -2.23 6.915 1.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "summitwave_dock_connector:MG0425BME"
		(layer "F.Cu")
		(uuid "86f5b3a2-e5ec-4351-9691-5afe92e09d23")
		(at 50.23 160.73)
		(property "Reference" "J3"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "3be3b949-b41e-4427-a9a8-0aeb1a8da98f")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "Conn_01x04"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "055e7ad4-33b0-4741-813e-fb6db9a6ddf9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5561ac40-3815-4b4d-a966-26eb48da1244")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "43d90ec8-f6e7-4081-a7eb-5edebee9883c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/ab4f7963-bcaa-45e5-90f9-2179b68e2f6b")
		(sheetname "/")
		(sheetfile "pcb_dock.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.61 -12.11)
			(end -0.23 -12.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9f549139-7a31-4b43-98b3-00129fc00d68")
		)
		(fp_line
			(start -1.61 -10.73)
			(end -1.61 -12.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "90cef198-389d-4f38-9640-60afd324019c")
		)
		(fp_line
			(start -1.61 -9.46)
			(end -1.61 -1.73)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6d374826-7c80-4661-8478-030a8229a7e3")
		)
		(fp_line
			(start -1.61 -9.46)
			(end 1.15 -9.46)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a84659f7-0198-4196-b3fd-f8f023abb4bb")
		)
		(fp_line
			(start -1.61 -1.73)
			(end 1.15 -1.73)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b1aece67-1860-4893-b2d0-c701acb77adb")
		)
		(fp_line
			(start 1.15 -9.46)
			(end 1.15 -1.73)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cdffd3ad-3f9b-4d9d-8306-8c1958d240af")
		)
		(fp_line
			(start -2 -12.5)
			(end -2 -1.34)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cfce8845-772b-46c8-bbd8-dce666db61cb")
		)
		(fp_line
			(start -2 -1.34)
			(end 1.54 -1.34)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3875f5eb-2df6-4af2-981c-7f88107f10ca")
		)
		(fp_line
			(start 1.54 -12.5)
			(end -2 -12.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "51520968-a73b-4a48-810e-528c89ac0767")
		)
		(fp_line
			(start 1.54 -1.34)
			(end 1.54 -12.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "600bbb29-83a2-431d-9b3c-f824c7105159")
		)
		(fp_line
			(start -1.5 -11.365)
			(end -0.865 -12)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "02ab8038-a9a3-4128-ab07-730374ea0a71")
		)
		(fp_line
			(start -1.5 -1.84)
			(end -1.5 -11.365)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ca28ee06-083c-484c-bf65-48e5c6237896")
		)
		(fp_line
			(start -0.865 -12)
			(end 1.04 -12)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f988e1a1-46af-4f98-8236-cc0c698e850f")
		)
		(fp_line
			(start 1.04 -12)
			(end 1.04 -1.84)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "06834c10-9feb-45e7-83cf-215814c352c6")
		)
		(fp_line
			(start 1.04 -1.84)
			(end -1.5 -1.84)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "10b1cec7-714c-4489-a269-58d63a21f7b0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "a6ee2c01-b40e-4353-9045-043bbd1f45a6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "${REFERENCE}"
			(at -0.23 -6.92 90)
			(layer "F.Fab")
			(uuid "fc00524c-8169-4177-9d2b-8b9ff3a36f09")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at -0.23 -10.73)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "bd1e4a1e-7bbe-43da-b54a-3fdf16cc23fd")
		)
		(pad "2" thru_hole circle
			(at -0.23 -8.19)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/A")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "ca95e6b4-bec6-4cb6-8486-54efa3748170")
		)
		(pad "3" thru_hole circle
			(at -0.23 -5.65)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/B")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "965eb429-366a-4491-be6e-6c185b90ba97")
		)
		(pad "4" thru_hole circle
			(at -0.23 -3.11)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "5498aa20-34fb-4c94-9797-166947cf79f6")
		)
		(embedded_fonts no)
		(embedded_files
			(file
				(name "MG0425BME.pdf")
				(type datasheet)
				(checksum "DDC9158D3DB55A592FB92759BC04B6F0")
			)
		)
		(model "${KIPRJMOD}/lib/MG0425BME.STEP"
			(offset
				(xyz -2.23 6.915 1.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "summitwave_dock_connector:MG0425BME"
		(layer "F.Cu")
		(uuid "997d1c7a-10da-4547-b023-f1bccefe3688")
		(at 110.23 160.73)
		(property "Reference" "J4"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "e5849c79-9cc6-499e-baf9-f6343b7426bf")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "Conn_01x04"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "3d823c8f-f0a2-437f-b440-6474ebf402c1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1c26c00b-ca49-48ca-8f37-28c57d59cd01")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8107c275-2ee0-408f-aa4a-cab3ca897420")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/63f36fcd-a210-4a1e-92d8-582e9db6a070")
		(sheetname "/")
		(sheetfile "pcb_dock.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.61 -12.11)
			(end -0.23 -12.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a5e033cb-0d8b-49ac-af57-e05638df616c")
		)
		(fp_line
			(start -1.61 -10.73)
			(end -1.61 -12.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1a0c0b05-c352-46db-bbb6-5576e78f1c9f")
		)
		(fp_line
			(start -1.61 -9.46)
			(end -1.61 -1.73)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7c93af37-1ee0-41ee-86b7-6f9cdf23176e")
		)
		(fp_line
			(start -1.61 -9.46)
			(end 1.15 -9.46)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "edc228b1-26dd-485c-82ef-6a4f89d1e5b5")
		)
		(fp_line
			(start -1.61 -1.73)
			(end 1.15 -1.73)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "67ba7e99-167c-4cbd-a96c-c6aae3abd347")
		)
		(fp_line
			(start 1.15 -9.46)
			(end 1.15 -1.73)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0852aecc-e537-4d7f-857c-d303bcf681b7")
		)
		(fp_line
			(start -2 -12.5)
			(end -2 -1.34)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "21de4b1d-dcab-4e0c-a4ca-681196a85390")
		)
		(fp_line
			(start -2 -1.34)
			(end 1.54 -1.34)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "205a6790-8c4f-48fd-9491-0f85f32903f6")
		)
		(fp_line
			(start 1.54 -12.5)
			(end -2 -12.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f04074e8-f0ea-465f-8438-b79390e16839")
		)
		(fp_line
			(start 1.54 -1.34)
			(end 1.54 -12.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "09a3924f-1a05-4360-a8bc-0343b49d07c6")
		)
		(fp_line
			(start -1.5 -11.365)
			(end -0.865 -12)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a45b169d-7197-4f74-a510-d6cc2c44427a")
		)
		(fp_line
			(start -1.5 -1.84)
			(end -1.5 -11.365)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8ec848ee-b249-49b3-8991-30a15d2d4d44")
		)
		(fp_line
			(start -0.865 -12)
			(end 1.04 -12)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1d3a5f4a-d810-40ca-bee1-3d88f38672a4")
		)
		(fp_line
			(start 1.04 -12)
			(end 1.04 -1.84)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1b9f4233-4bf8-4324-9d78-7f714e29a479")
		)
		(fp_line
			(start 1.04 -1.84)
			(end -1.5 -1.84)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c979a321-3f70-4f06-abf8-6bb1a9805f17")
		)
		(fp_text user "${REFERENCE}"
			(at -0.23 -6.92 90)
			(layer "F.Fab")
			(uuid "452e56c8-bfa8-4de1-8205-c53fb46be46c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "605ce1da-53df-4921-bd78-bc7b2b0359b8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at -0.23 -10.73)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "9a5de9f5-d26e-4191-b693-92f76b227a8c")
		)
		(pad "2" thru_hole circle
			(at -0.23 -8.19)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/A")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "8252fdf1-208a-4b91-bc38-dd9c80107b25")
		)
		(pad "3" thru_hole circle
			(at -0.23 -5.65)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/B")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "6a58a78b-223f-41e7-b8f9-a0d4a190ee17")
		)
		(pad "4" thru_hole circle
			(at -0.23 -3.11)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "d57d83f9-685b-4f2e-bb2e-cb2ea7aa19d1")
		)
		(embedded_fonts no)
		(embedded_files
			(file
				(name "MG0425BME.pdf")
				(type datasheet)
				(checksum "DDC9158D3DB55A592FB92759BC04B6F0")
			)
		)
		(model "${KIPRJMOD}/lib/MG0425BME.STEP"
			(offset
				(xyz -2.23 6.915 1.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "lcsc_lib:SOIC-8_L5.0-W4.0-P1.27-LS6.0-BL"
		(layer "F.Cu")
		(uuid "9cd231e0-f167-4dec-bdb1-94ef57831710")
		(at 24.728418 96.695)
		(property "Reference" "U2"
			(at 0 -6.71 0)
			(layer "F.SilkS")
			(uuid "c8116e23-be95-45c4-bb37-f2968e779f44")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SP485EEN-L/TR"
			(at 0 6.71 0)
			(layer "F.Fab")
			(uuid "00c521ae-b692-4741-ba4c-78b56c2d98d1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://lcsc.com/product-detail/RS-485-RS-422_SIPEX_SP485EEN-L-TR_SP485EEN-L-TR_C6855.html"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6c2fa535-5dcd-4f86-8c8c-ba8baf7ebc09")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "143096a5-d8a2-4093-b1ec-0139be9a18a4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC Part" "C6855"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6c79bf9c-db11-4adc-ba8d-868646237782")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/8d54e627-c356-4951-aebe-3144a8fa65f3")
		(sheetname "/")
		(sheetfile "pcb_dock.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.5 -1.5)
			(end -2.5 -0.73)
			(stroke
				(width 0.25)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "04022eab-0246-417e-ae05-bef0d3b9895c")
		)
		(fp_line
			(start -2.5 -1.5)
			(end 2.5 -1.5)
			(stroke
				(width 0.25)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bea6cd2a-4a66-497b-8cd4-1cd3cff31392")
		)
		(fp_line
			(start -2.5 1.5)
			(end -2.5 0.73)
			(stroke
				(width 0.25)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a410ed56-d34d-4fbd-a113-a515e536f9d8")
		)
		(fp_line
			(start -2.5 1.5)
			(end 2.5 1.5)
			(stroke
				(width 0.25)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2afc152d-5db2-4f8b-b45a-903d73d728e7")
		)
		(fp_line
			(start 2.5 -1.5)
			(end 2.5 1.5)
			(stroke
				(width 0.25)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9578f250-7b5c-4c46-8286-5edfa36ae691")
		)
		(fp_arc
			(start -2.48726 -0.729889)
			(mid -2.50637 0.729972)
			(end -2.5 -0.73)
			(stroke
				(width 0.25)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "99d81b66-b47f-49fa-820e-5810c08d8f08")
		)
		(fp_circle
			(center -1.78 1.02)
			(end -1.63 1.02)
			(stroke
				(width 0.3)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "b7556085-e974-4ba0-b70e-be7038e4c090")
		)
		(fp_circle
			(center -1.91 3.4)
			(end -1.76 3.4)
			(stroke
				(width 0.3)
				(type solid)
			)
			(fill no)
			(layer "Cmts.User")
			(uuid "64c1cbb0-ed42-4b8f-8a5e-09a511a2b7ec")
		)
		(fp_circle
			(center -2.41 3)
			(end -2.38 3)
			(stroke
				(width 0.06)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "77dda876-444f-4a0d-9f3a-8a4421397191")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "ebfb5b28-3290-40c9-be1e-a5438079c02a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd oval
			(at -1.91 2.71)
			(size 0.57 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "Net-(U1-RXD)")
			(pinfunction "RO")
			(pintype "unspecified")
			(uuid "0dcba90e-593a-4f86-950b-b116b329c7d4")
		)
		(pad "2" smd oval
			(at -0.63 2.71)
			(size 0.57 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(U1-CBUS3)")
			(pinfunction "~{RE}")
			(pintype "unspecified")
			(uuid "a4628af4-52c7-4de5-ac9b-7f434ee4bb30")
		)
		(pad "3" smd oval
			(at 0.63 2.71)
			(size 0.57 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U1-CBUS2)")
			(pinfunction "DE")
			(pintype "unspecified")
			(uuid "a9235212-8760-49c3-a69a-1eb44ce44ce4")
		)
		(pad "4" smd oval
			(at 1.9 2.71)
			(size 0.57 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(U1-TXD)")
			(pinfunction "DI")
			(pintype "unspecified")
			(uuid "4d3cfc13-1c7f-4627-a6f4-20c79d2f387e")
		)
		(pad "5" smd oval
			(at 1.9 -2.71)
			(size 0.57 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "unspecified")
			(uuid "378c7fa0-c99a-46bf-b2f8-ae34c59a6fed")
		)
		(pad "6" smd oval
			(at 0.63 -2.71)
			(size 0.57 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "/A")
			(pinfunction "A")
			(pintype "unspecified")
			(uuid "64dc8a40-dd98-47ab-b92c-90db9d171c75")
		)
		(pad "7" smd oval
			(at -0.63 -2.71)
			(size 0.57 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/B")
			(pinfunction "B")
			(pintype "unspecified")
			(uuid "4d42102e-a587-48bc-b980-308430b3d7a2")
		)
		(pad "8" smd oval
			(at -1.91 -2.71)
			(size 0.57 1.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "+5V")
			(pinfunction "VCC")
			(pintype "unspecified")
			(uuid "05ae1b34-ed97-43f5-aed3-c055620fb4cc")
		)
		(embedded_fonts no)
		(model "/lcsc_lib.3dshapes/SOIC-8_L5.0-W4.0-P1.27-LS6.0-BL.wrl"
			(offset
				(xyz 0 -0 -0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/lib/lcsc_lib.3dshapes/SOIC-8_L5.0-W4.0-P1.27-LS6.0-BL.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric"
		(layer "F.Cu")
		(uuid "dae1bd1f-8218-4d41-a3e8-e3387a971ea0")
		(at 85.9375 100)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "FB1"
			(at 0 -1.55 0)
			(layer "F.SilkS")
			(uuid "77407301-31fc-485b-9dfb-57e3090a77a3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "FerriteBead"
			(at 0 1.55 0)
			(layer "F.Fab")
			(uuid "febe023d-a5e4-4340-9f2b-7601fb5b7d01")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8fcb957a-698c-4a36-a97d-fe16fc3f9593")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Ferrite bead"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d78f84a9-1eb8-49ce-a55c-dfc0e2698d1c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C74764"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b81457eb-90de-4f22-b394-22b19fc94893")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(path "/22f882da-b5af-43a8-8e00-338b33e670f7")
		(sheetname "/")
		(sheetfile "pcb_dock.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.399622 -0.56)
			(end 0.399622 -0.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "55f00100-d196-4631-8041-c576240e379a")
		)
		(fp_line
			(start -0.399622 0.56)
			(end 0.399622 0.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cfe9cede-1d01-4aff-a77f-981290c4c6ad")
		)
		(fp_line
			(start -1.75 -0.85)
			(end 1.75 -0.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "072f31c5-3fe1-4df6-a4b5-6d42318f29e4")
		)
		(fp_line
			(start -1.75 0.85)
			(end -1.75 -0.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "758e65ff-dbcc-414c-9570-f740c601fc1c")
		)
		(fp_line
			(start 1.75 -0.85)
			(end 1.75 0.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6b3d7297-16e7-4823-a831-a912dbfe5345")
		)
		(fp_line
			(start 1.75 0.85)
			(end -1.75 0.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "551fea2d-6cbe-4c49-8503-6b4d7d6e87bc")
		)
		(fp_line
			(start -1 -0.45)
			(end 1 -0.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eb281be3-8401-427d-89fd-d9fa8d9ffd48")
		)
		(fp_line
			(start -1 0.45)
			(end -1 -0.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8b3cb482-0fd4-42aa-9292-e8b5963d29bf")
		)
		(fp_line
			(start 1 -0.45)
			(end 1 0.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "68c1d4d0-5d6c-4d55-84c8-832a65dccc45")
		)
		(fp_line
			(start 1 0.45)
			(end -1 0.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fef6422a-c575-48b3-945d-194f83f56bed")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "46e1a1f9-4516-412b-83f0-afb96fdeb532")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0625 0)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "unconnected-(FB1-Pad1)")
			(pintype "passive")
			(uuid "60245da2-beaa-4b4a-8fb7-f0d0d38d2581")
		)
		(pad "2" smd roundrect
			(at 1.0625 0)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "unconnected-(FB1-Pad2)")
			(pintype "passive")
			(uuid "8c68e372-160c-4ae7-a125-9db50321eecf")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(embedded_fonts no)
	(embedded_files
		(file
			(name "MG0425BME.pdf")
			(type datasheet)
			(data |KLUv/aAOqAIArLAP/O0eJVBERi0xLjcNCiWhs8XXDQo4IDAgb2JqDQo8PC9MZW5ndGggMjc1Nzkv
[encoded data, 242433 characters]
				8fk4aB9/I2QbX5Z1/D7odsoXKs04N+DLm1SdQfqrsYRkSIWyHHUxFPmrAg==|
			)
			(checksum "DDC9158D3DB55A592FB92759BC04B6F0")
		)
	)
)
