(footprint "MG0425BME"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "feeb7080-09fd-4e39-8309-ca579f4da7c9")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "MG0425BME"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "5fe0abfa-14b5-489d-954b-73188ae1af00")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "kicad-embed://MG0425BME.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c2e8ca2e-ed4c-46e0-846b-8429fa31faa4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a21102bb-52ee-4e45-83e1-78dc6af76204")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.61 -12.11)
		(end -0.23 -12.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "22cef716-2104-45b0-8cde-e37b31d89b69")
	)
	(fp_line
		(start -1.61 -10.73)
		(end -1.61 -12.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5505e122-ba18-4703-9797-8ee45e208eb3")
	)
	(fp_line
		(start -1.61 -9.46)
		(end -1.61 -1.73)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c455e951-fa42-4e27-b640-8f0dbb1cbc99")
	)
	(fp_line
		(start -1.61 -9.46)
		(end 1.15 -9.46)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6e526776-0bfa-472f-813b-0fe6794678b2")
	)
	(fp_line
		(start -1.61 -1.73)
		(end 1.15 -1.73)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "95af1280-e7aa-4e12-b257-3fc2e5e0d0bf")
	)
	(fp_line
		(start 1.15 -9.46)
		(end 1.15 -1.73)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8086624a-0a8c-4f3a-b1a7-5ba1705ab47b")
	)
	(fp_line
		(start -2 -12.5)
		(end -2 -1.34)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "9d66800b-c693-4645-8832-24356e484862")
	)
	(fp_line
		(start -2 -1.34)
		(end 1.54 -1.34)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f72c827b-7dd7-402a-9c67-1c57889c51e1")
	)
	(fp_line
		(start 1.54 -12.5)
		(end -2 -12.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "dcd3e83e-efdc-45e7-9ace-0dfa4912c278")
	)
	(fp_line
		(start 1.54 -1.34)
		(end 1.54 -12.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e5b93422-38eb-4183-ae14-d1bf474f0ca9")
	)
	(fp_line
		(start -1.5 -11.365)
		(end -0.865 -12)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0fb727ca-48d5-46d6-9d70-6d95ead97009")
	)
	(fp_line
		(start -1.5 -1.84)
		(end -1.5 -11.365)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c8c9141b-c20d-4a9d-9ba5-bc3dfd99929f")
	)
	(fp_line
		(start -0.865 -12)
		(end 1.04 -12)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d7e3512c-6a8e-41d4-a772-76311b25bf6c")
	)
	(fp_line
		(start 1.04 -12)
		(end 1.04 -1.84)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2baea055-7653-42b0-ab20-0a83c6a54ed5")
	)
	(fp_line
		(start 1.04 -1.84)
		(end -1.5 -1.84)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9f2da751-0939-4966-8312-c9bd83968289")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "6a51dd9c-4a34-456d-a6fd-ea1e6401ec58")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at -0.23 -6.92 90)
		(layer "F.Fab")
		(uuid "ad72b748-9410-41c9-938e-a863757db6cd")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at -0.23 -10.73)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1ef0a496-3a12-400f-8902-4742716c37b4")
	)
	(pad "2" thru_hole circle
		(at -0.23 -8.19)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "78687224-294d-4d6c-a729-511343b0506a")
	)
	(pad "3" thru_hole circle
		(at -0.23 -5.65)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "534e86ef-bc06-4886-8293-f5cc2caa6ef5")
	)
	(pad "4" thru_hole circle
		(at -0.23 -3.11)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e0a80ba1-1563-4843-8471-1e4847e56880")
	)
	(embedded_fonts no)
	(embedded_files
		(file
			(name "MG0425BME.pdf")
			(type datasheet)
			(data |KLUv/aAOqAIArLAP/O0eJVBERi0xLjcNCiWhs8XXDQo4IDAgb2JqDQo8PC9MZW5ndGggMjc1Nzkv
[encoded data, 242433 characters]
				8fk4aB9/I2QbX5Z1/D7odsoXKs04N+DLm1SdQfqrsYRkSIWyHHUxFPmrAg==|
			)
			(checksum "DDC9158D3DB55A592FB92759BC04B6F0")
		)
	)
	(model "${KIPRJMOD}/lib/MG0425BME.STEP"
		(offset
			(xyz -2.23 6.915 1.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 -0 -90)
		)
	)
)
