(module easyeda2kicad:SOIC-8_L5.0-W4.0-P1.27-LS6.0-BL (layer F.Cu) (tedit 5DC5F6A4)
	(attr smd)
	(fp_text reference REF** (at 0 -6.71) (layer F.SilkS)
		(effects (font (size 1 1) (thickness 0.15)))
	)
	(fp_text value SOIC-8_L5.0-W4.0-P1.27-LS6.0-BL (at 0 6.71) (layer F.Fab)
		(effects (font (size 1 1) (thickness 0.15)))
	)
	(fp_text user %R (at 0 0) (layer F.Fab)
		(effects (font (size 1 1) (thickness 0.15)))
	)
	(fp_line (start -2.50 1.50) (end 2.50 1.50) (layer F.SilkS) (width 0.25))
	(fp_line (start -2.50 -1.50) (end 2.50 -1.50) (layer F.SilkS) (width 0.25))
	(fp_line (start -2.50 1.50) (end -2.50 0.73) (layer F.SilkS) (width 0.25))
	(fp_line (start -2.50 -1.50) (end -2.50 -0.73) (layer F.SilkS) (width 0.25))
	(fp_line (start 2.50 -1.50) (end 2.50 1.50) (layer F.SilkS) (width 0.25))
	(pad 1 smd oval (at -1.91 2.71 0.00) (size 0.57 1.95) (layers F.Cu F.Paste F.Mask))
	(pad 2 smd oval (at -0.63 2.71 0.00) (size 0.57 1.95) (layers F.Cu F.Paste F.Mask))
	(pad 3 smd oval (at 0.63 2.71 0.00) (size 0.57 1.95) (layers F.Cu F.Paste F.Mask))
	(pad 4 smd oval (at 1.90 2.71 0.00) (size 0.57 1.95) (layers F.Cu F.Paste F.Mask))
	(pad 8 smd oval (at -1.91 -2.71 0.00) (size 0.57 1.95) (layers F.Cu F.Paste F.Mask))
	(pad 7 smd oval (at -0.63 -2.71 0.00) (size 0.57 1.95) (layers F.Cu F.Paste F.Mask))
	(pad 6 smd oval (at 0.63 -2.71 0.00) (size 0.57 1.95) (layers F.Cu F.Paste F.Mask))
	(pad 5 smd oval (at 1.90 -2.71 0.00) (size 0.57 1.95) (layers F.Cu F.Paste F.Mask))
	(fp_circle (center -2.41 3.00) (end -2.38 3.00) (layer F.Fab) (width 0.06))
	(fp_circle (center -1.91 3.40) (end -1.76 3.40) (layer Cmts.User) (width 0.30))
	(fp_circle (center -1.78 1.02) (end -1.63 1.02) (layer F.SilkS) (width 0.30))
	(fp_arc (start -2.50 0.00) (end -2.50 -0.73) (angle -359.00) (layer F.SilkS) (width 0.25))
	(model "/lcsc_lib.3dshapes/SOIC-8_L5.0-W4.0-P1.27-LS6.0-BL.wrl"
		(offset (xyz 0.000 -0.000 -0.000))
		(scale (xyz 1 1 1))
		(rotate (xyz 0 0 0))
	)
)