(kicad_symbol_lib
  (version 20211014)
  (generator https://github.com/uPesy/easyeda2kicad.py)
  (symbol "FT232RL-REEL"
    (in_bom yes)
    (on_board yes)
    (property
      "Reference"
      "U"
      (id 0)
      (at 0 33.02 0)
      (effects (font (size 1.27 1.27) ) )
    )
    (property
      "Value"
      "FT232RL-REEL"
      (id 1)
      (at 0 -33.02 0)
      (effects (font (size 1.27 1.27) ) )
    )
    (property
      "Footprint"
      "lcsc_lib:SSOP-28_L10.2-W5.3-P0.65-LS7.8-BL"
      (id 2)
      (at 0 -35.56 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (property
      "Datasheet"
      "https://lcsc.com/product-detail/USB_FTDI_FT232RL-REEL_FT232RL-REEL_C8690.html"
      (id 3)
      (at 0 -38.10 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (property
      "LCSC Part"
      "C8690"
      (id 5)
      (at 0 -40.64 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (symbol "FT232RL-REEL_0_1"
      (rectangle
        (start -17.78 22.86)
        (end 17.78 -22.86)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin unspecified line
        (at 22.86 -20.32 180)
        (length 5.08)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 22.86 -17.78 180)
        (length 5.08)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line
        (at 2.54 27.94 270)
        (length 5.08)
        (name "VCCIO" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 22.86 17.78 180)
        (length 5.08)
        (name "RXD" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 22.86 2.54 180)
        (length 5.08)
        (name "RI" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line
        (at 0.00 -27.94 90)
        (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 22.86 12.70 180)
        (length 5.08)
        (name "DSR" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 22.86 5.08 180)
        (length 5.08)
        (name "DCD" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 22.86 7.62 180)
        (length 5.08)
        (name "CTS" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line
        (at 22.86 -12.70 180)
        (length 5.08)
        (name "CBUS4" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line
        (at 22.86 -7.62 180)
        (length 5.08)
        (name "CBUS2" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line
        (at 22.86 -10.16 180)
        (length 5.08)
        (name "CBUS3" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line
        (at -22.86 7.62 0)
        (length 5.08)
        (name "USBDP" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line
        (at -22.86 12.70 0)
        (length 5.08)
        (name "USBDM" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin output line
        (at -22.86 20.32 0)
        (length 5.08)
        (name "3V3OUT" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line
        (at 2.54 -27.94 90)
        (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -22.86 -2.54 0)
        (length 5.08)
        (name "RESET" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line
        (at -2.54 27.94 270)
        (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line
        (at 5.08 -27.94 90)
        (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line
        (at 22.86 -5.08 180)
        (length 5.08)
        (name "CBUS1" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line
        (at 22.86 -2.54 180)
        (length 5.08)
        (name "CBUS0" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line
        (at -5.08 -27.94 90)
        (length 5.08)
        (name "AGND" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -22.86 -20.32 0)
        (length 5.08)
        (name "TEST" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -22.86 -7.62 0)
        (length 5.08)
        (name "OSCI" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin output line
        (at -22.86 -15.24 0)
        (length 5.08)
        (name "OSCO" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin output line
        (at 22.86 20.32 180)
        (length 5.08)
        (name "TXD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line
        (at 22.86 15.24 180)
        (length 5.08)
        (name "DTR" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line
        (at 22.86 10.16 180)
        (length 5.08)
        (name "RTS" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SP485EEN-L_TR"
    (in_bom yes)
    (on_board yes)
    (property
      "Reference"
      "U"
      (id 0)
      (at 0 8.89 0)
      (effects (font (size 1.27 1.27) ) )
    )
    (property
      "Value"
      "SP485EEN-L/TR"
      (id 1)
      (at 0 -8.89 0)
      (effects (font (size 1.27 1.27) ) )
    )
    (property
      "Footprint"
      "lcsc_lib:SOIC-8_L5.0-W4.0-P1.27-LS6.0-BL"
      (id 2)
      (at 0 -11.43 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (property
      "Datasheet"
      "https://lcsc.com/product-detail/RS-485-RS-422_SIPEX_SP485EEN-L-TR_SP485EEN-L-TR_C6855.html"
      (id 3)
      (at 0 -13.97 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (property
      "LCSC Part"
      "C6855"
      (id 5)
      (at 0 -16.51 0)
      (effects (font (size 1.27 1.27) ) hide)
    )
    (symbol "SP485EEN-L_TR_0_1"
      (rectangle
        (start -5.08 6.35)
        (end 5.08 -6.35)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin unspecified line
        (at -10.16 3.81 0)
        (length 5.08)
        (name "RO" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -10.16 1.27 0)
        (length 5.08)
        (name "~{RE}" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -10.16 -1.27 0)
        (length 5.08)
        (name "DE" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at -10.16 -3.81 0)
        (length 5.08)
        (name "DI" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 10.16 -3.81 180)
        (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 10.16 -1.27 180)
        (length 5.08)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 10.16 1.27 180)
        (length 5.08)
        (name "B" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line
        (at 10.16 3.81 180)
        (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
)